iServer (Commands Received):

1. Start : SRT IP:PORT (e.g. SRT [10.10.90.09:00090])
2. Add : ADD “file name” (e.g. ADD [10.10.90.09:00090][ReadMe.txt])
3. Remove : REM “file name” (e.g. REM [10.10.90.09:00090][ReadMe.txt])
4. Close : CLO (e.g. CLO [10.10.90.09:00090])
5. Search : SRC “file name” (e.g. SRC [ReadMe.txt])

Node (Commands Received):

1. Search Results : SRCHRES [ip:port::ip:port::ip:port]
2. Get : GET [file name]
3. Get Reply : GRPY [No of Segments][Port]
4. File Transfer : FTRAN [segment data